**COUNTY PERFERRED TOUCH-FREE RESTROOM FIXTURES & DOOR LOCKS**

**(OR - AS APPROVED EQUAL)**

**Faucets**

**SLOAN® SENSOR FAUCET - CODE NUMBER 3362115 (HARD WIRED)**

<https://www.sloan.com/spec-sheet/3362115>

**SLOAN® SENSOR FAUCET -CODE NUMBER 3362118 (BATTERY POWERED)**

<https://www.sloan.com/spec-sheet/3362118>

**Water Closets (Toilets)**

**ROYAL® SENSOR FLUSHOMETER - CODE NUMBER 3010065**

<https://www.sloan.com/spec-sheet/3010065>

**ROYAL® SENSOR FLUSHOMETER - CODE NUMBER 3910058**

<https://www.sloan.com/spec-sheet/3910058>

**8000C Concealed Retrofit Urinal & Toilet Flush Valve**

<https://hydrotekintl.com/product/8000c-concealed-retrofit-urinal-toilet-flush-valve/> (in wall battery/ Hard Wire powered)

<https://www.hydrotekintl.com/wp-content/uploads/2011/02/O-M-Hydrotek-model-H-8000C.pdf>

**Urinal**

**ROYAL® SENSOR FLUSHOMETER - CODE NUMBER 3912679**

<https://www.sloan.com/spec-sheet/3912679>

**Bottle Fillers**

**Indoor Rated**

**Elkay EZH2O Bottle Filling Station Surface Mount Non-Filtered Non-Refrigerated Stainless Model EZWSSM**

<http://www.elkayfiles.com/spec-sheets/ezwssm_spec.pdf>

**Outdoor rated**

M-OBR4 Wall Mounted Recessed Bottle Filler with Cover Plate, Sensor and Push Button

<https://murdockoutdoorfountains.com/M-OBR4>

<https://www.murdockmfg.com/uploads/fileLibrary/MOBR4.pdf>

**Hand Dryer**

**XLERATOReco® HAND DRYER**

<https://www.exceldryer.com/product/xleratoreco-hand-dryer/>

<https://www.exceldryer.com/wp-content/uploads/2019/12/XLERATOReco-Tech-Sheet.pdf>

**Valve Commode (For Tank Flush Replacement)**

**ELONGATED FLOOR-MOUNTED ADA WATER CLOSET ST-2029**

<https://www.sloan.com/spec-sheet/2102029>

**Auto Timer Door Locks**

Metal Door Frames, Hinges, Closers and Push / Pull Plate replacement may vary depending on location.  These items will be at the contractor’s discretion to provide quality and a secured facility.

Best Access Door Lever

<https://www.bestaccess.com/files/9814/6179/9584/9Kseries_WEB.pdf>

Electric Strike 5200C 12-24VAC/VDC 2004M 630 –

<https://content.assaabloyusa.com/doc/AADSS1058531&.pdf>

<https://content.assaabloyusa.com/doc/AADSS1053610&.pdf>

**Power Supply**

<https://www.assaabloyesh.com/Local/assaabloyeshCOM/Securitron/_OWNA2.0/Documents/Installation_Instructions/Power_Supplies/AQ%20Series%20Power%20Supply%20Manuals/500-25010_1%20AQD%20Manual.pdf>

**Timer**

<https://www.assaabloyesh.com/Local/assaabloyeshCOM/Securitron/_OWNA2.0/Documents/Installation_Instructions/Access_Control_Accessories/DT-7_IO_500-11800_D.pdf>

**Best Access ADA Compliant Deadbolt 8T Series**

<https://www.bestaccess.com/files/1014/6183/3660/Tseries_BAS014_WEB.pdf>

Or as Approved Equal Occupancy Indicator, ADA compliant thumb turn Deadbolt